## Comet parameter: minimum_intensity

- A floating point number indicating the minimum intensity value for input the input peaks.
- If an experimental MS/MS peak intensity is less than this value, it will not be read in and used in the analysis.
- This is one mechanism to get rid of systemmatic background noise that has a near contant peak intensity.
- If a peak does not pass this minimum intensity threshold, it will also not be counted towards the minimum_peaks parameter.
- Valid values are any floating point number.
- The default value is "0.0" if this parameter is missing.

Example:
`minimum_intensity = 100.0`